Ch10 :

10 – 40 Wi-Fi setup

Connect a laptop to SOHO router with an Ethernet cable

使用乙太網路線將筆記型電腦連接到 SOHO 路由器

乙太網路連接至路由器後再連接至所需WIFI裝置

Use a browser to access the router home page

使用瀏覽器存取路由器首頁

使用瀏覽器設置路由器資訊

Change admin password and SSID; also add security

更改管理者密碼和SSID；還增加安全性

10 – 41 Going high speed

Wired, wireless, and cellular connections provide high-speed Internet

有線、無線和蜂窩連接提供高速互聯網

有線無線(行動網路)能夠提供速度快的聯網

Wired connections offer the best overall performance

有線連接提供最佳的整體性能

有線除了行動性之外 其他都優於無線

Cellular connections provide best mobility

蜂窩連接提供最佳的移動性

行動網路提供最佳的移動性

10 – 42 Setting up and sharing printers

Install printer drivers and assure good connectivity

安裝印表機驅動程式並確保良好的連接

要安裝驅動程式才能用哦

Devices and Printers | Printer Properties | Print a test page

設備和印表機|印表機屬性 |列印測試頁

看起來應該是測試印表機是否安裝成功

Printer Properties | Sharing | Share this printer

印表機屬性 |分享|共用這台印表機

如何多台連線印表機?

Which on of the following describes the probability that a system will be functional?

下列哪一項描述了系統正常運作的機率？

Availability(可用性)

Which of the following is NOT a type of high-speed internet connection?

下列何者不屬於高速網路連線類型？

Edge(邊緣)

Which high-speed internet connection allows the most concurrent users?

哪種高速網路連線允許最多的並發用戶？

Cellular(行動網路)

This is one of the most important steps when configuring a new SOHO router.

這是配置新 SOHO 路由器時最重要的步驟。

Change the default admin password(更改預設管理員密碼)

Where do you go to install a printer in Windows, especially in Windows 8 and previous versions?

在 Windows 中，尤其是在 Windows 8 及之前的版本中，您應該在哪裡安裝印表機？

Control Panel(控制台)

Once a printer is installed, how do you make sure it is working?

安裝印表機後，如何確保其正常運作？

Print a test page.(打印測試文件)

What device do you need to create a wired network?

創建有線網路需要什麼設備？

Switch(交換器)

When there are more people attempting to access the internet than the WAP can, then the WAP has reached its \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ limit.

當嘗試上網的人數多於 WAP 所能容納的人數時，WAP 就已達到其 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 限制。

Concurrent users(並發用戶)